**Firmware version 2.1:**

* Removed delays in transmit function, otherwise identical to fw version 2.0

**Firmware version 3.0:**

* Firmware now automatically detects when the positioner is finished with a move, move times will no longer need to be added to post-pauses
* ‘SYNC’ has been changed from active-low to active-high
* FW version formatting has been expanded to two bytes
* ADC readout of current monitors has been added (no timing of readout yet)
* Fiducial command has been split into two: one command to select between the fiducial functionality and positioner functionality and a second command to set the duty cycle.